

GPIO_PIN_DHT = 4 # BCM
SENSORDATA_URL = 'http://tfm.meteor.com/api/v1.0/sensorData'
GPIO_PIN_TANKFULL = 20 # BCM
GPIO_PIN_OUT_VALVE = 21 # BCM
GPIO_PIN_IN_VALVE = 18 # BCM
API_BASE_URL = 'http://tfm.meteor.com/api/v1.0'
CONTROLLER_ID = '120' # every controller must have a different one
STATE_FILE = '/var/run/controller_state'
